.\" $XFree86$
.TH GTF 1 __vendorversion__
.SH NAME
gtf - calculate VESA GTF mode lines
.SH SYNOPSIS
.B gtf
.I h-resolution
.I v-resolution
.I refresh
.RB [ \-v | \-\-verbose ]
.RB [ \-f | \-\-fbmode ]
.RB [ \-x | \-\-xorgmode ]
.SH DESCRIPTION
.I Gtf
is a utility for calculating VESA GTF modes.  Given the desired
horizontal and vertical resolutions and refresh rate (in Hz), the parameters
for a matching VESA GTF mode are printed out.  Two output formats are
supported: mode lines suitable for the __xservername__
.B __xconfigfile__(__filemansuffix__)
file, and mode parameters suitable for the Linux
.B fbset(8)
utility.

.SH OPTIONS
.TP 8
.BR \-v | \-\-verbose
Enable verbose printouts  This shows a trace for each step of the
computation.
.TP 8
.BR \-x | \-\-xorgmode
Print the mode parameters as __xservername__-style mode lines.  This is the
default format.
.TP 8
.BR \-f | \-\-fbset
Print the mode parameters in a format suitable for
.BR fbset(8) .
.SH "SEE ALSO"
__xconfigfile__(__filemansuffix__)
.SH AUTHOR
Andy Ritger.
.PP
This program is based on the Generalized Timing Formula (GTF(TM)) Standard
Version: 1.0, Revsion: 1.0.  The GTF Excel(TM) spreadsheet, a sample
(and the definitive) implementation of the GTF Timing Standard is
available at <ftp://ftp.vesa.org/pub/GTF/VTF_V1R1.xls>.
