# $XFree86: xc/programs/Xserver/hw/xfree98/xf86config/Cards98,v 1.7 1998/06/04 16:43:45 hohndel Exp $
#
#
#
# $XConsortium: Cards /main/27 1996/10/28 05:43:53 kaleb $
# This is the database of card definitions used by xf86config.
# Each definition should have a NAME entry, CHIPSET (descriptive) and
# SERVER (one of EGC, GANBWAP, PEGC, NKVNEC, WABS, WABEP, WSNA, TGUI,
# MGA, SVGA, NECS3, PWSKB, PWLB, GA968).
# A reference to another definition is made with SEE (already defined
# entries are not overridden).
# Optional entries are RAMDAC (identifier), CLOCKCHIP (identifier),
# DACSPEED, NOCLOCKPROBE (advises never to probe clocks), UNSUPPORTED
# (indicates card that is not yet properly supported by a dedicated
# server). A LINE entry adds a line of text to be included in the
# Device section (can include options or comments).
# There's no CLOCKS option (although a Clocks line can be included
# with LINE), as it is very undesirable to have a Clocks line that
# is incorrect. The idea is that the Clocks are probed for to be
# sure (a commented suggested Clocks line can be included).
#
# The majority of entries are just a binding of a model name to a
# chipset/server and untested.
#

# EGC

NAME EGC16
CHIPSET EGC
SERVER EGC
LINE    Chipset "vga"

# PEGC

NAME PEGC
CHIPSET PEGC
SERVER PEGC
LINE    VideoRam	512
LINE    Clocks	31.5
LINE    # Virtual resolution for 640x400
LINE    # Clocks	28.322

# GANBWAP

NAME GA-98NBI
CHIPSET CL-GD5434
SERVER GANBWAP
LINE    ClockChip	"cirrus"
LINE    Option	"ga98nb1"
LINE    Option	"no_mmio"
LINE    # Option	"sw_cursor"

NAME GA-98NBII
CHIPSET CL-GD5434
SERVER GANBWAP
LINE    ClockChip	"cirrus"
LINE    Option	"ga98nb2"
LINE    Option	"no_mmio"
LINE    # Option	"sw_cursor"

NAME GA-98NBIV
CHIPSET CL-GD5434
SERVER GANBWAP
LINE    ClockChip	"cirrus"
LINE    Option	"ga98nb4"
LINE    Option	"no_mmio"
LINE    # Option	"sw_cursor"

NAME WAP-2000/4000
CHIPSET CL-GD5434
SERVER GANBWAP
LINE    Option	"wap"
LINE    Option	"no_mmio"
LINE    # Option	"epsonmemwin"

# NKVNEC

NAME PCNKV/PCNKV2/NEC_CIRRUS
CHIPSET CL-GD5428/5429/5430
SERVER NKVNEC
LINE    # Option	"fast_dram"
LINE    VideoRam    1024

NAME PC9821Bf/U8W
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Bp/U8W/U7W
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Bs/U7W
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Be/U7W
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821BA3/U2/W
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821BX3/U2/W
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821BX4/U2
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Cb
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Ce
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Cf
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Ce2
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Cs
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Cs2
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Cx
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Cx2
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Es
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Nd
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Ne2
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Nf
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Np
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Ns
LINE    Option	"nec_cirrus"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821V7/C
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821V10/C,S
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821V12/S
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821V13/S
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821V16/S
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821V16/S5V,P
LINE    Chipset "clgd5446"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821V20/S7
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Xb10
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Xc13/S5
LINE    Chipset "clgd5446"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Xc16/M,S
LINE    Chipset "clgd5446"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Xc200/M,S
LINE    Chipset "clgd5446"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Xa7e
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Xe
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC9821Xe10
LINE    Chipset "clgd5430"
LINE    Option	"nec_cirrus"
LINE    Option	"no_mmio"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC486MR
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC486MS
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC486MU
LINE    Chipset "clgd5429"
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC486MV
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC586MV
SEE PCNKV/PCNKV2/NEC_CIRRUS

NAME PC586RV
LINE    Chipset "clgd5429"
SEE PCNKV/PCNKV2/NEC_CIRRUS

# WABS

NAME WAB-S
CHIPSET CL-GD5426/5428
SERVER WABS
LINE    VideoRam	1024
LINE    # VideoRam	2048

NAME WAB-1000/2000
CHIPSET CL-GD5428
SERVER WABS
LINE    VideoRam	1024
LINE    # VideoRam	2048

NAME WSR-E/G
SEE WAB-1000/2000

# WABEP

NAME WAB-EP
CHIPSET CL-GD5428
SERVER WABEP
LINE    Option	"med_dram"

# WSNA

NAME WSN-A2F
CHIPSET CL-GD5434
SERVER WSNA
LINE    Option	"no_mmio"
LINE    Option	"med_dram"

# TGUI

NAME NEC Trident
CHIPSET TGUI9680/9682
SERVER TGUI
LINE    Option	"xaa_no_color_exp"
LINE    # Option	"noaccel"
LINE    # Option	"Linear"
LINE    # Option	"med_dram"
LINE    # Option	"hw_cursor"

NAME PC9821Ra20/N
SEE NEC Trident

NAME PC9821RaII23/N,W
SEE NEC Trident

NAME PC9821Ra266/N,W
SEE NEC Trident

NAME PC9821Rs20/B20
SEE NEC Trident

NAME PC9821RsII26/B40
SEE NEC Trident

NAME PC9821V13/M7
SEE NEC Trident

NAME PC9821V16/M7
SEE NEC Trident

NAME PC9821V20/M7
SEE NEC Trident

NAME PC9821Xa7/C,K
SEE NEC Trident

NAME PC9821Xa9/C,K
SEE NEC Trident

NAME PC9821Xa10/C,K
SEE NEC Trident

NAME PC9821Xa12/C,K
SEE NEC Trident

NAME PC9821Xa13/C,K,W
SEE NEC Trident

NAME PC9821Xa16/R,W
SEE NEC Trident

NAME PC9821Xa20/W
SEE NEC Trident

NAME PC9821Xc13/M,S
SEE NEC Trident

NAME PC9821Xv13/R
SEE NEC Trident

NAME GA-DRV/98
CHIPSET TGUI9680
SERVER TGUI
LINE    Option	"noaccel"
LINE    # Option	"med_dram"
LINE    # Option	"hw_cursor"

# MGA

NAME MGA Millennium
CHIPSET MGA2064W
SERVER MGA

NAME PC9821Xt13
SEE MGA Millennium

NAME PC9821Xt16
SEE MGA Millennium

NAME PC9821Xv13/W
SEE MGA Millennium

NAME PC9821Xv20/W
SEE MGA Millennium

NAME PC9821St15
SEE MGA Millennium

NAME PC9821St20
SEE MGA Millennium

NAME PC9821RvII26/N20
SEE MGA Millennium

NAME NEC FC-WAB-X2
SEE MGA Millennium

NAME MGA Mystique
CHIPSET MGA1064SG
SERVER MGA

NAME PC9821V166/S
LINE    VideoRam	2048
SEE MGA Mystique

NAME PC9821V200/S
LINE    VideoRam	2048
SEE MGA Mystique

NAME PC9821V200/M
LINE    VideoRam	4096
SEE MGA Mystique

NAME PC9821V233/M7
LINE    VideoRam	2048
SEE MGA Mystique

NAME PC9821V233/M7V
LINE    VideoRam	4096
SEE MGA Mystique

# SVGA

NAME NEC Cirrus 755x
CHIPSET CL-GD7555
LINE    Chipset "clgd7555"
LINE    # VideoRam	2048
LINE    # Option	"no_bitblt"
LINE    # Option	"fast_dram"
LINE    Option	"linear"
LINE    Option	"noaccel"
SERVER SVGA

NAME PC9821Nr12
SEE NEC Cirrus 755x

NAME PC9821Nr13
SEE NEC Cirrus 755x

NAME PC9821La13
SEE NEC Cirrus 755x

NAME PC9821Ls12
SEE NEC Cirrus 755x

NAME PC9821Ls13
SEE NEC Cirrus 755x

NAME PC9821Ls150
SEE NEC Cirrus 755x

# NECS3

NAME NEC WAB-A/B
CHIPSET S3 928
SERVER NECS3
LINE    Chipset	"s3_generic"
LINE    Dacspeed	110
LINE    Ramdac	"sc15025"
LINE    Option	"dac_8_bit"
LINE    # Option	"necwab"
LINE    # Option	"nomemaccess"
LINE    Clocks	25.0  28.0  40.0   0.0  50.0  77.0  36.0  45.0
LINE    Clocks	130.0 120.0  80.0  31.0 110.0  65.0  75.0  94.0

NAME NEC FC-WAB-A/B
CHIPSET S3 928
SERVER NECS3
LINE    Chipset	"s3_generic"
LINE    Dacspeed	110
LINE    Ramdac	"bt485"
LINE    Option	"necwab"
LINE    Option	"nomemaccess"
LINE    Option	"noinit"
LINE    Option	"nolinear"
LINE    Clocks	25.0  28.0  40.0   0.0  50.0  77.0  36.0  45.0
LINE    Clocks	130.0 120.0  80.0  31.0 110.0  65.0  75.0  94.0

NAME PC9821Af/U9W E09?
SEE NEC WAB-A/B

NAME PC9821An/U8W
SEE NEC WAB-A/B

NAME PC9821Ap2/U8W/C9W
SEE NEC WAB-A/B

NAME PC9821As2/U7W/U8W
SEE NEC WAB-A/B

NAME NEC 864
CHIPSET S3 864
SERVER NECS3
LINE    Chipset	"s3_generic"
LINE    Option	"necwab"
LINE    Ramdac	"s3_sdac"
LINE    ClockChip	"s3_sdac"

NAME PC9821Ap3
SEE NEC 864

NAME PC9821As3
SEE NEC 864

NAME PC9821Xp
SEE NEC 864

NAME PC9821Xs
SEE NEC 864

# PWSKB

NAME PowerWindow 928/801
CHIPSET S3 928
SERVER PWSKB
LINE    Chipset	"s3_generic"
LINE    # Chipset	"mmio_928"
LINE    Ramdac	"sc15025"
LINE    Dacspeed	110
LINE    Option	"dac_8_bit"
LINE    # Option	"epsonmemwin"
LINE    # Option	"nomemaccess"
LINE    ClockChip	"icd2061a"

NAME PowerWindow 928II
CHIPSET S3 928
SERVER PWSKB
LINE    Chipset	"s3_generic"
LINE    # Chipset	"mmio_928"
LINE    Ramdac	"att20c505"
LINE    # Ramdac	"bt485"
LINE    Dacspeed	110
LINE    Option	"dac_8_bit"
LINE    # Option	"pw_mux"
LINE    Option	"bt485_curs"
LINE    # Option	"epsonmemwin"
LINE    # Option	"nomemaccess"
LINE    ClockChip	"icd2061a"

NAME PowerWindow 805i
CHIPSET S3 805
SERVER PWSKB
LINE    Chipset	"s3_generic"
LINE    Ramdac	"s3gendac"
LINE    Dacspeed	110
LINE    Option	"dac_8_bit"
LINE    # Option	"pw805i"
LINE    # Option	"epsonmemwin"
LINE    # Option	"nomemaccess"
LINE    ClockChip	"s3_sdac"

NAME PowerWindow 928G
CHIPSET S3 928
SERVER PWSKB
LINE    Chipset	"s3_generic"
LINE    # Chipset	"mmio_928"
LINE    Ramdac	"sc15025"
LINE    Dacspeed	110
LINE    Option	"dac_8_bit"
LINE    # Option	"nomemaccess"
LINE    # Option	"nolinear"
LINE    ClockChip	"icd2061a"

NAME PCSKB/PCSKB2
CHIPSET S3 911/924
SERVER PWSKB
LINE    Chipset	"s3_generic"
LINE    Ramdac	"sc15025"
LINE    Dacspeed	110
LINE    Option	"dac_8_bit"
LINE    # Option	"nomemaccess"
LINE    Option	"pcskb"
LINE    Clocks	25.0  28.0  40.0   0.0  50.0  77.0  36.0  45.0
LINE    Clocks	130.0 120.0  80.0  31.0 110.0  65.0  75.0  94.0

NAME PCSKB3/PCSKB4/PCPKB4
CHIPSET S3 928
SERVER PWSKB
LINE    Chipset	"s3_generic"
LINE    Ramdac	"sc15025"
LINE    # Ramdac	"att20c498"
LINE    Dacspeed	110
LINE    Option	"dac_8_bit"
LINE    Option	"nomemaccess"
LINE    Option	"pcskb4"
LINE    Clocks	 25.0  28.0  40.0   0.0  50.0  77.0  36.0  45.0
LINE    Clocks	130.0 120.0  80.0  31.0 110.0  65.0  75.0  94.0

# PWLB

NAME PowerWindow 928GLB
CHIPSET S3 928
SERVER PWLB
LINE    Chipset	"s3_generic"
LINE    # Chipset	"mmio_928"
LINE    Ramdac	"sc15025"
LINE    Dacspeed	110
LINE    Option	"dac_8_bit"
LINE    # Option	"pw_localbus"
LINE    # Option	"nomemaccess"
LINE    # Option	"nolinear"
LINE    ClockChip	"icd2061a"

NAME PowerWindow 928IILB
CHIPSET S3 928
SERVER PWLB
LINE    Chipset	"s3_generic"
LINE    # Chipset	"mmio_928"
LINE    Ramdac	"att20c505"
LINE    # Ramdac	"bt485"
LINE    Dacspeed	110
LINE    Option	"dac_8_bit"
LINE    Option	"bt485_curs"
LINE    Option	"pw_localbus"
LINE    # Option	"pw_mux"
LINE    # Option	"nomemaccess"
LINE    # Option	"nolinear"
LINE    ClockChip	"icd2061a"

NAME PowerWindow 964LB
CHIPSET S3 964
SERVER PWLB
LINE    Chipset	"s3_generic"
LINE    Option	"pw_localbus"
LINE    Option	"number_nine"
LINE    Ramdac	"ti3025"
LINE    ClockChip	"ti3025"
LINE    VideoRam	4096

# GA968

NAME GA-968V4/PCI
CHIPSET S3 968
SERVER GA968
LINE    Chipset	"s3_generic"
LINE    # Chipset	"mmio_928"
LINE    VideoRam	4096
