# $XConsortium: Cards /main/27 1996/10/28 05:43:53 kaleb $
# This is the database of card definitions used by xf86config.
# Each definition should have a NAME entry, CHIPSET (descriptive) and
# SERVER (one of Mono, VGA16, SVGA, S3, 8514, Mach8, Mach32, Mach64, AGX,
# P9000, W32, I128).
# A reference to another definition is made with SEE (already defined
# entries are not overridden).
# Optional entries are RAMDAC (identifier), CLOCKCHIP (identifier),
# DACSPEED, NOCLOCKPROBE (advises never to probe clocks), UNSUPPORTED
# (indicates card that is not yet properly supported by a dedicated
# server). A LINE entry adds a line of text to be included in the
# Device section (can include options or comments).
# There's no CLOCKS option (although a Clocks line can be included
# with LINE), as it is very undesirable to have a Clocks line that
# is incorrect. The idea is that the Clocks are probed for to be
# sure (a commented suggested Clocks line can be included).
#
# The majority of entries are just a binding of a model name to a
# chipset/server and untested.
#
# $XFree86: xc/programs/Xserver/hw/xfree86/xf86config/Cards,v 3.79 2002/10/16 01:31:05 dawes Exp $

# VGA

NAME * Generic VGA compatible
SERVER VGA16
DRIVER vga

NAME * Generic VESA compatible
SERVER VGA16
DRIVER vesa

NAME * Unsupported VGA compatible
SERVER VGA16
DRIVER vga
UNSUPPORTED


#	  #
# generic #
#	  #

NAME ** Alliance Pro Motion (generic)      [apm]
#CHIPSET apm
SERVER SVGA
DRIVER apm
LINE #Option "no_accel"

NAME ** Ark Logic (generic)                [ark]
#CHIPSET ark
SERVER SVGA
DRIVER ark

NAME ** ASPEED Technology (generic)        [ast]
#CHIPSET ast
SERVER SVGA
DRIVER ast

NAME ** ATI (generic)                      [ati]
#CHIPSET ati
SERVER SVGA
DRIVER ati

NAME ** ATI Rage 128 based (generic)       [r128]
#CHIPSET r128
SERVER SVGA
DRIVER r128

NAME ** ATI Radeon (generic)               [radeon]
#CHIPSET radeon
SERVER SVGA
DRIVER radeon

NAME ** Chips and Technologies (generic)   [chips]
#CHIPSET chips
SERVER SVGA
DRIVER chips
LINE # Option "suspend_hack"
LINE # Option "STN"
LINE # Option "no_stretch"
LINE # Option "no_center"
LINE # Option "use_modeline"
LINE # Option "fix_panel_size"
LINE # videoram 512
LINE # Option "noaccel"
LINE # Option "no_bitblt"
LINE # Option "xaa_no_color_exp"
LINE # Option "xaa_benchmark"
LINE # Option "hw_cursor"
LINE # Option "nolinear"
LINE # MemBase 0x03b00000
LINE # Option "hw_clocks"
LINE # Textclockfreq 25.175

NAME ** Cirrus Logic (generic)             [cirrus]
#CHIPSET cirrus
SERVER SVGA
DRIVER cirrus
LINE # MemBase 0x00e00000		# ISA card that maps to 14Mb
LINE # MemBase 0x04000000		# VLB card that maps to 64Mb
LINE # MemBase 0x80000000		# VLB card that maps to 2048Mb
LINE # MemBase 0x02000000		# VLB card that maps to 32Mb
LINE # Option "linear"
LINE # Option "fifo_conservative"

NAME ** Cyrix MediaGX (generic)            [cyrix]
#CHIPSET cyrix
SERVER SVGA
DRIVER cyrix

NAME ** Linux framebuffer (generic)        [fbdev]
#CHIPSET fbdev
SERVER SVGA
DRIVER fbdev

NAME ** 3DLabs, TI (generic)               [glint]
#CHIPSET glint
SERVER SVGA
DRIVER glint
LINE #Option "no_accel"

NAME ** Number Nine I128 (generic)         [i128]
#CHIPSET i128
SERVER SVGA
DRIVER i128

NAME ** Intel i740 (generic)               [i740]
#CHIPSET i740
SERVER SVGA
DRIVER i740

NAME ** Intel i810 (generic)               [i810]
#CHIPSET i810
SERVER SVGA
DRIVER i810

NAME ** Matrox Graphics (generic)          [mga]
#CHIPSET mga
SERVER SVGA
DRIVER mga
LINE # Option "mga_sdram"

NAME ** NeoMagic (generic)                 [neomagic]
#CHIPSET neomagic
SERVER SVGA
DRIVER neomagic
LINE # Chipset    "NM2160"
LINE # IOBase     0xfea00000
LINE # MemBase    0xfd000000
LINE # VideoRam   2048
LINE # DacSpeed   90
LINE # Option     "linear"
LINE # Option     "nolinear"
LINE # Option     "sw_cursor"
LINE # Option     "hw_cursor"
LINE # Option     "no_accel"
LINE # Option     "intern_disp"
LINE # Option     "extern_disp"
LINE # Option     "mmio"
LINE # Option     "no_mmio"
LINE # Option     "lcd_center"
LINE # Option     "no_stretch"

NAME ** NVIDIA (generic)                   [nv]
#CHIPSET nv
SERVER SVGA
DRIVER nv

NAME ** Rendition (generic)                [rendition]
#CHIPSET rendition
SERVER SVGA
DRIVER rendition
LINE # Option "sw_cursor"

NAME ** S3 (not ViRGE or Savage) (generic) [s3]
#CHIPSET s3
SERVER SVGA
DRIVER s3

NAME ** S3 ViRGE (generic)                 [s3virge]
#CHIPSET s3virge
SERVER SVGA
DRIVER s3virge
LINE # Option "xaa_benchmark"
LINE # Option "fifo_moderate"
LINE # Option "pci_burst_on"
LINE # Option "pci_retry"
LINE # Option "lcd_center"
LINE # Set_LCDClk  <pixel_clock_for_LCD>

NAME ** S3 Savage (generic)                [savage]
#CHIPSET savage
SERVER SVGA
DRIVER savage

NAME ** Silicon Motion (generic)           [siliconmotion]
#CHIPSET siliconmotion
SERVER SVGA
DRIVER siliconmotion

NAME ** SiS (generic)                      [sis]
#CHIPSET sis
SERVER SVGA
DRIVER sis
LINE # Option "no_accel"
LINE # Option "fifo_moderate"
LINE # Option "fifo_conserv"
LINE # Option "fifo_aggressive"
LINE # Option "no_BitBlt"
LINE # Option "fast_vram"
LINE # Option "pci_burst_on"
LINE # Option "xaa_benchmark"
LINE # Option "ext_eng_queue"

NAME ** 3Dfx (generic)                     [tdfx]
#CHIPSET tdfx
SERVER SVGA
DRIVER tdfx

NAME ** DEC TGA (generic)                  [tga]
#CHIPSET tga
SERVER SVGA
DRIVER tga

NAME ** Trident (generic)                  [trident]
#CHIPSET trident
SERVER SVGA
DRIVER trident

NAME ** Tseng Labs (generic)               [tseng]
#CHIPSET tseng
SERVER SVGA
DRIVER tseng
LINE # Option "linear"
LINE # Option "noaccel"
LINE # Option "power_saver"
LINE # Option "fast_dram"
LINE # Option "pci_retry"
LINE # Option "hibit_high"
LINE # Option "hibit_low"
LINE # MemBase 0x3C00000

NAME ** VMWare guest OS (generic)          [vmware]
#CHIPSET vmware
SERVER SVGA
DRIVER vmware


#Chips & Technologies

#untested
NAME Chips & Technologies CT65520
CHIPSET ct65520
SERVER SVGA
DRIVER chips
LINE # Device section for C&T cards.
LINE # Option "suspend_hack"
LINE # Option "STN"
LINE # Option "no_stretch"
LINE # Option "no_center"
LINE # Option "use_modeline"
LINE # Option "fix_panel_size"
LINE # videoram 512

NAME Chips & Technologies CT65525
CHIPSET ct65525
LINE # Option "nolinear"
LINE # MemBase 0x03b00000
SEE Chips & Technologies CT65520

NAME Chips & Technologies CT65530
CHIPSET ct65530
SEE Chips & Technologies CT65525

NAME Chips & Technologies CT65535
CHIPSET ct65535
NOCLOCKPROBE
LINE # Option "hw_clocks"
LINE # Textclockfreq 25.175
SEE Chips & Technologies CT65530

NAME Chips & Technologies CT65540
CHIPSET ct65540
NOCLOCKPROBE
LINE # Option "use_18bit_bus"
SEE Chips & Technologies CT65535

NAME Chips & Technologies CT65545
CHIPSET ct65545
NOCLOCKPROBE
LINE # Option "noaccel"
LINE # Option "no_bitblt"
LINE # Option "xaa_no_color_exp"
LINE # Option "xaa_benchmark"
LINE # Option "hw_cursor"
LINE # Option "mmio"
SEE Chips & Technologies CT65540

NAME Chips & Technologies CT65546
CHIPSET ct65546
SEE Chips & Technologies CT65545

NAME Chips & Technologies CT65548
CHIPSET ct65548
SEE Chips & Technologies CT65545

NAME Chips & Technologies CT65550
CHIPSET ct65550
NOCLOCKPROBE
LINE # Option "noaccel"
LINE # Option "no_bitblt"
LINE # Option "xaa_no_color_exp"
LINE # Option "xaa_benchmark"
LINE # Option "hw_cursor"
LINE # Option "sync_on_green"
LINE # Option "fast_dram"
LINE # Option "use_vclk1"
LINE # Textclockfreq 25.175
SEE Chips & Technologies CT65530

NAME Chips & Technologies CT65554
CHIPSET ct65554
SEE Chips & Technologies CT65550

NAME Chips & Technologies CT65555
CHIPSET ct65555
SEE Chips & Technologies CT65550

NAME Chips & Technologies CT68554
CHIPSET ct68554
SEE Chips & Technologies CT65550

NAME Chips & Technologies CT69000
CHIPSET ct69000
SEE Chips & Technologies CT65550

NAME Chips & Technologies CT69030
CHIPSET ct69030
SEE Chips & Technologies CT65550

NAME Chips & Technologies CT64200
CHIPSET ct64200
SERVER SVGA
DRIVER chips
LINE # Device section for C&T cards.
LINE # videoram 1024

NAME Chips & Technologies CT64300
CHIPSET ct64300
SERVER SVGA
DRIVER chips
LINE # Option "noaccel"
LINE # Option "no_bitblt"
LINE # Option "xaa_no_color_exp"
LINE # Option "xaa_benchmark"
LINE # Option "hw_cursor"
LINE # Option "nolinear"
LINE # MemBase 0x03b00000
LINE # Option "hw_clocks"
LINE # Textclockfreq 25.175
SEE Chips & Technologies CT64200

# Cirrus Logic

#tested
NAME Cirrus Logic GD542x
SERVER SVGA
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE
LINE # Device section for Cirrus Logic GD5420/2/4/6/8/9-based cards.
LINE     #MemBase 0x00e00000
LINE     #MemBase 0x04e00000
LINE     #Option "linear"

#tested
NAME Cirrus Logic GD543x
CHIPSET CL-GD5430/5434/5436
SERVER SVGA
DRIVER cirrus
NOCLOCKPROBE
LINE # Device section for Cirrus Logic GD5430/34-based cards.
LINE     #MemBase 0x00e00000		# ISA card that maps to 14Mb
LINE     #MemBase 0x04000000		# VLB card that maps to 64Mb
LINE     #MemBase 0x80000000		# VLB card that maps to 2048Mb
LINE     #MemBase 0x02000000		# VLB card that maps to 32Mb
LINE     #Option "linear"

NAME Cirrus Logic GD544x
CHIPSET CL-GD544x
SERVER SVGA
DRIVER cirrus
NOCLOCKPROBE

NAME Creative Labs Graphics Blaster MA201
SEE Cirrus Logic GD544x

NAME Creative Labs Graphics Blaster MA202
SEE Cirrus Logic GD544x

#tested
NAME Cirrus Logic GD5462
CHIPSET CL-GD5462
SERVER SVGA
DRIVER cirrus
NOCLOCKPROBE
LINE #Option "fifo_conservative"

#tested
NAME Cirrus Logic GD5464
CHIPSET CL-GD5464
SERVER SVGA
DRIVER cirrus
NOCLOCKPROBE
LINE #Option "fifo_conservative"

#tested
NAME Cirrus Logic GD5465
CHIPSET CL-GD5465
SERVER SVGA
DRIVER cirrus
NOCLOCKPROBE
LINE #Option "fifo_conservative"

NAME Creative Labs Graphics Blaster MA302
CHIPSET CL-GD5462
SEE Cirrus Logic GD5462

NAME Creative Labs Graphics Blaster MA334
CHIPSET CL-GD5464
SEE Cirrus Logic GD5464

NAME Creative Labs Graphics Blaster 3D
CHIPSET CL-GD5464
SEE Cirrus Logic GD5464

#tested
NAME Cirrus Logic GD5480
CHIPSET CL-GD5480
SERVER SVGA
DRIVER cirrus
NOCLOCKPROBE

#tested
NAME Diamond SpeedStar 64
CHIPSET CL-GD5434
SEE Cirrus Logic GD543x

NAME Diamond SpeedStar64 Graphics 2000/2200
CHIPSET CL-GD5434
SEE Cirrus Logic GD543x

NAME Diamond SpeedStar Pro SE (CL-GD5430/5434)
SEE Cirrus Logic GD543x

NAME Diamond SpeedStar Pro 1100
SEE Cirrus Logic GD542x

NAME Orchid Kelvin 64 VLB Rev A
CHIPSET CL-GD5434
SERVER SVGA
DRIVER cirrus
NOCLOCKPROBE
LINE # Device section for Orchid Kelvin 64 VLB Rev A
LINE # Linear framebuffer maps at 2048Mb. Some motherboards make linear addressing
LINE # impossible. Some cards map at 32Mb.
LINE     #MemBase 0x02000000		# VLB card that maps to 32Mb
LINE     #MemBase 0x04000000		# VLB card that maps to 64Mb
LINE     MemBase 0x80000000		# VLB card that maps to 2048Mb
LINE     #Option "linear"

NAME Orchid Kelvin 64 VLB Rev B
CHIPSET CL-GD5434
SERVER SVGA
DRIVER cirrus
NOCLOCKPROBE
LINE # Device section for Orchid Kelvin 64 VLB Rev B
LINE # Linear framebuffer maps at 32Mb. Some motherboards make linear addressing
LINE # impossible. Some cards map at 2048Mb.
LINE     MemBase 0x02000000		# VLB card that maps to 32Mb
LINE     #MemBase 0x04000000		# VLB card that maps to 64Mb
LINE     #MemBase 0x80000000		# VLB card that maps to 2048Mb
LINE     #Option "linear"

NAME Orchid Kelvin 64
CHIPSET CL-GD5434
SEE Cirrus Logic GD543x

NAME Intel 5430
CHIPSET CL-GD5430
SEE Cirrus Logic GD543x

NAME STB Nitro (64)
CHIPSET CL-GD5434
SEE Cirrus Logic GD543x

NAME STB Nitro 64 Video
CHIPSET CL-GD5446
SEE Cirrus Logic GD544x

NAME STB Horizon
CHIPSET CL-GD5426/28
SEE Cirrus Logic GD542x

NAME STB Horizon Video
CHIPSET CL-GD5440
SEE Cirrus Logic GD544x

NAME Genoa 8500VL(-28)
CHIPSET CL-GD5426/28
SEE Cirrus Logic GD542x

NAME Diamond SpeedStar Pro (not SE)
CHIPSET CL-GD5426/28
SEE Cirrus Logic GD542x

NAME ALG-5434(E)
CHIPSET CL-GD5434
SEE Cirrus Logic GD543x

NAME Actix ProStar
CHIPSET CL-GD5426/5428
SEE Cirrus Logic GD542x

NAME Actix ProStar 64
CHIPSET CL-GD5434
SEE Cirrus Logic GD543x

#tested
NAME Acumos AVGA3
SEE Cirrus Logic GD542x

NAME DFI-WG1000
SEE Cirrus Logic GD542x

NAME Spider VLB Plus
CHIPSET CL-GD5428
SEE Cirrus Logic GD542x

NAME VI720
CHIPSET CL-GD5434
SEE Cirrus Logic GD543x

NAME Cirrus Logic GD62xx (laptop)
CHIPSET CL-GD6205/15/25/35
SERVER SVGA
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME Cirrus Logic GD64xx (laptop)
CHIPSET CL-GD6420/6440
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Cirrus Logic GD754x (laptop)
CHIPSET CL-GD7541/42/43/48
SERVER SVGA
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME Techworks Ultimate 3D
CHIPSET CL-GD5464
SEE Cirrus Logic GD5464

NAME VideoLogic GrafixStar 550
CHIPSET CL-GD5464
SEE Cirrus Logic GD5464

NAME Jaton Video-70P
CHIPSET CL-GD5464
SEE Cirrus Logic GD5464

NAME PixelView Combo TV Pro (Prolink)
CHIPSET CL-GD5480, 4MB
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE # COMMENT on card TV Tuner
NOCLOCKPROBE

NAME PixelView Combo TV 3D AGP (Prolink)
CHIPSET CL-GD5465, 4MB
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE # COMMENT on card TV+FM Tuner
NOCLOCKPROBE

NAME Creative Labs Graphics Blaster Eclipse (OEM Model CT6510)
SEE Cirrus Logic GD5465

NAME VideoLogic GrafixStar 560 (PCI/AGP)
SEE Cirrus Logic GD5465

NAME Cirrus Logic GD5446 (noname card)
CHIPSET CL-GD5446, 1MB (upgradable to 2MB).
SERVER SVGA
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME Octek VL-VGA-26
CHIPSET CL-GD5426
SEE Cirrus Logic GD542x

NAME Octek VL-VGA-28
CHIPSET CL-GD5428
SEE Cirrus Logic GD542x

NAME Octek Combo-26
CHIPSET CL-GD5426
SEE Cirrus Logic GD542x

NAME Octek Combo-28
CHIPSET CL-GD5428
SEE Cirrus Logic GD542x

NAME Octek AVGA-20
SEE Cirrus Logic GD542x

# S3 801/805

NAME S3 801/805 (generic)
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED

NAME S3 86C801 (generic)
SEE S3 801/805 (generic)

NAME S3 86C805 (generic)
SEE S3 801/805 (generic)

#tested
NAME S3 801/805 with ATT20c490 RAMDAC
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c490
LINE     #Option "dac_8_bit"		# Not supported by some 20c490 clones

NAME S3 801/805 with SC1148{2,3,4} RAMDAC
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC sc11482

NAME S3 801/805 with SC1148{5,7,9} RAMDAC
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC sc11485

NAME S3 801/805 with S3 GenDAC
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC s3gendac
CLOCKCHIP s3gendac

NAME S3 801/805 with ATT20c490 RAMDAC and ICD2061A
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c490
CLOCKCHIP icd2061a
LINE     #Option "dac_8_bit"		# Not supported by some 20c490 clones

NAME S3 801/805 with Chrontel 8391
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c490
CLOCKCHIP ch8391
LINE     Option "dac_8_bit"

#tested
NAME Actix GE32+ 2MB
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c490
LINE     #Option "dac_8_bit"

NAME Actix GE32i
CHIPSET S3 805i
SERVER S3
DRIVER vga
UNSUPPORTED

NAME Orchid Fahrenheit VA
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c490

NAME Orchid Fahrenheit 1280
CHIPSET S3 801
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Probable clocks:
LINE     #Clocks 25.20 28.32 32.50 0.00 40.00 44.90 50.40 65.00
LINE     #Clocks 78.00 56.70 63.10 75.10 80.00 89.90 100.90 31.50

NAME Orchid Fahrenheit-1280+
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20C490
LINE     Dacspeed   110
LINE     Option     "dac_8_bit"
LINE     #Option    "nolinear" # VLB card may require this
LINE     #Probable clocks:
LINE     #Clocks     25.20 28.32 40.0 0.0 50.10 77.0 36.10 45.0
LINE     #Clocks     130.0 120.20 80.0 31.50 110.30 65.0 75.0 94.60

NAME Diamond Stealth 24
CHIPSET S3 801/805
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2061a
LINE     #Option    "nolinear"
LINE     #Ramdac "att20c490" # The Diamond RAMDAC is reportedly compatible for 15bpp

NAME Miro Crystal 8S
SEE S3 801/805 (generic)

NAME Miro Crystal 10SD with GenDAC
SEE S3 801/805 with S3 GenDAC

NAME Dell S3 805
SEE S3 801/805 (generic)

NAME STB Powergraph X-24
SEE S3 801/805 with ATT20c490 RAMDAC and ICD2061A

NAME JAX 8241
SEE S3 801/805 with Chrontel 8391

NAME VL-41
SEE S3 801/805 with Chrontel 8391

NAME SPEA Mirage
SEE S3 801/805 with Chrontel 8391

# S3 864/Trio64/Trio32/868

NAME S3 864 (generic)
SERVER S3
DRIVER vga
UNSUPPORTED

NAME S3 86C864 (generic)
SEE S3 864 (generic)

NAME S3 Vision864 (generic)
SEE S3 864 (generic)

NAME S3 864 with SDAC (86C716)
CHIPSET S3 864
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC s3_sdac
CLOCKCHIP s3_sdac
NOCLOCKPROBE

NAME S3 864 with ATT 20C498 or 21C498
CHIPSET S3 864
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c498

NAME S3 864 with STG1703
CHIPSET S3 864
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC stg1703
NOCLOCKPROBE

NAME S3 868 (generic)
CHIPSET S3 868
SERVER S3
DRIVER vga
UNSUPPORTED

NAME S3 86C868 (generic)
SEE S3 868 (generic)

NAME S3 Vision868 (generic)
SEE S3 868 (generic)

NAME S3 868 with SDAC (86C716)
CHIPSET S3 868
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME S3 868 with ATT 20C498 or 21C498
CHIPSET S3 868
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c498

NAME S3 868 with ATT 20C409
CHIPSET S3 868
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c409
NOCLOCKPROBE

NAME Number Nine FX Motion 531
CLOCKCHIP icd2061a
SEE S3 868 with ATT 20C498 or 21C498

NAME S3 Trio64 (generic)
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME S3 86C764 (generic)
SEE S3 Trio64 (generic)

NAME S3 Trio64V+ (generic)
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME S3 86C765 (generic)
SEE S3 Trio64V+ (generic)

NAME S3 Trio32 (generic)
CHIPSET S3 Trio32
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME Genoa Phantom 64i with S3 SDAC
DACSPEED 135
SEE S3 864 with SDAC (86C716)

NAME Number Nine GXE64
CHIPSET S3 864
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2061a
LINE     Option "number_nine"

NAME Number Nine GXE64 with S3 Trio64
SEE S3 Trio64 (generic)

NAME Diamond Stealth 64 DRAM with S3 SDAC
DACSPEED 135
SEE S3 864 with SDAC (86C716)

NAME Diamond Stealth64 Graphics 2xx0 series (864 + SDAC)
DACSPEED 135
SEE S3 864 with SDAC (86C716)

NAME Diamond Stealth 64 DRAM with S3 Trio64
SEE S3 Trio64 (generic)

NAME Diamond Stealth64 Graphics 2xx0 series (Trio64)
SEE S3 Trio64 (generic)

NAME Diamond Stealth 64 DRAM SE
SEE S3 Trio32 (generic)

NAME Diamond Stealth64 Video 2001 series (2121/2201)
SEE S3 Trio64V+ (generic)

NAME Actix GE64
CLOCKCHIP icd2061a
SEE S3 864 (generic)

NAME ELSA Winner 1000PRO with S3 SDAC
SEE S3 864 with SDAC (86C716)

NAME ELSA Winner 1000PRO with STG1700 or AT&T RAMDAC
CHIPSET S3 864
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2061a

NAME ELSA Winner 1000PRO/X
SEE S3 868 with SDAC (86C716)

NAME ELSA Winner 1000ISA
CHIPSET S3 805i
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2061a
LINE     Option "dac_8_bit"
LINE     # the following settings should be detected and set automatically by XF86_S3
LINE     # if the serial number of the ELSA card is printed correctly:
LINE     #ClockChip "icd2061a"

NAME Cardex Trio64
SEE S3 Trio64 (generic)

NAME Cardex Trio64Pro
SEE S3 Trio64 (generic)

NAME Miro Crystal 12SD
SEE S3 Trio32 (generic)

NAME Miro Crystal 22SD
SEE S3 Trio64 (generic)

NAME Miro Crystal 20SD with ICS2494 (BIOS 1.xx)
SEE S3 864 with ATT 20C498 or 21C498

NAME Miro Crystal 20SD with ICD2061A (BIOS 2.xx)
CLOCKCHIP icd2061a
SEE S3 864 with ATT 20C498 or 21C498

NAME Miro Crystal 20SD VLB with S3 SDAC (BIOS 3.xx)
SEE S3 864 with SDAC (86C716)

NAME Miro Crystal 20SD PCI with S3 SDAC
SEE S3 868 with SDAC (86C716)

NAME ELSA Winner 1000AVI (SDAC version)
SEE S3 868 with SDAC (86C716)

NAME ELSA Winner 1000AVI (AT&T 20C409 version)
SEE S3 868 with ATT 20C409

NAME Diamond Stealth Video DRAM
SEE S3 868 with SDAC (86C716)

NAME Diamond Stealth64 Video 2120/2200
SEE S3 868 with SDAC (86C716)

NAME SPEA/V7 Mirage P64
CLOCKCHIP ics2595
SEE S3 864 (generic)

NAME SPEA/V7 Mirage P64 with S3 Trio64
SEE S3 Trio64 (generic)

NAME Number Nine FX Vision 330
SEE S3 Trio64 (generic)

NAME Number Nine FX Motion 331
SEE S3 Trio64V+ (generic)

NAME ASUS Video Magic PCI V864
SEE S3 864 (generic)

NAME ASUS Video Magic PCI VT64
SEE S3 Trio64 (generic)

NAME VidTech FastMax P20
SEE S3 864 (generic)

NAME VideoLogic GrafixStar 500
SEE S3 868 with SDAC (86C716)

NAME VideoLogic GrafixStar 400
SEE S3 Trio64V+ (generic)

NAME VideoLogic GrafixStar 300
SEE S3 Trio64 (generic)

NAME 2 the Max MAXColor S3 Trio64V+
SEE S3 Trio64V+ (generic)

NAME DataExpert DSV3365
SEE S3 Trio64V+ (generic)

NAME ExpertColor DSV3365
SEE S3 Trio64V+ (generic)

NAME DSV3326
SEE S3 Trio64V+ (generic)

# S3 Trio64V2

NAME S3 Trio64V2 (generic)
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME S3 Trio64V2/DX (generic)
SEE S3 Trio64V2 (generic)

NAME S3 Trio64V2/GX (generic)
SEE S3 Trio64V2 (generic)

NAME S3 86C775 (generic)
SEE S3 Trio64V2/DX (generic)

NAME S3 86C785 (generic)
SEE S3 Trio64V2/GX (generic)

NAME ELSA WINNER 1000/T2D
SEE S3 Trio64V2/DX (generic)


# S3 Aurora64V+

NAME S3 Aurora64V+ (generic)
CHIPSET S3 Aurora64V+
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE
LINE     # Option "lcd_center"
LINE     # Set_LCDClk  <pixel_clock_for_LCD>

NAME S3 86CM65
SEE S3 Aurora64V+ (generic)

NAME SHARP 9080
SEE S3 Aurora64V+ (generic)

NAME SHARP 9090
SEE S3 Aurora64V+ (generic)

NAME COMPAQ Armada 7730MT
SEE S3 Aurora64V+ (generic)

NAME COMPAQ Armada 7380DMT
SEE S3 Aurora64V+ (generic)


# S3 964/968

NAME S3 964 (generic)
CHIPSET S3 964
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME S3 86C964 (generic)
SEE S3 964 (generic)

NAME S3 Vision964 (generic)
SEE S3 964 (generic)

NAME S3 968 (generic)
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME S3 86C968 (generic)
SEE S3 968 (generic)

NAME S3 Vision968 (generic)
SEE S3 968 (generic)

NAME Number Nine GXE64 Pro
CHIPSET S3 964
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC ti3025
LINE     Option "number_nine"

NAME Diamond Stealth 64 VRAM
CLOCKCHIP icd2061a
LINE    #Option "slow_vram"
SEE S3 964 (generic)

NAME Diamond Stealth64 Video 3200
CHIPSET S3 968
LINE    #Option "slow_vram"
SEE S3 968 (generic)

NAME Diamond Stealth 64 Video VRAM (TI RAMDAC)
CHIPSET S3 968
LINE    #Option "slow_vram"
LINE    #DacSpeed 220
SEE S3 968 (generic)

NAME Diamond Stealth64 Video 3240/3400 (TI RAMDAC)
CHIPSET S3 968
LINE    #Option "slow_vram"
LINE    #DacSpeed 220
SEE S3 968 (generic)

NAME Diamond Stealth64 Video 3240/3400 (IBM RAMDAC)
CHIPSET S3 968
LINE    #Option "slow_vram"
RAMDAC ibm_rgb526
LINE    DacSpeed 220
SEE S3 968 (generic)

NAME Genoa VideoBlitz III AV
CHIPSET S3 968
LINE    #s3RefClk  50
LINE    #DACspeed 170
SEE S3 968 (generic)

NAME STB Velocity 64 Video
CHIPSET S3 968
LINE    #s3RefClk  24
LINE    #DACspeed 220
SEE S3 968 (generic)

NAME STB Powergraph 64 Video
SEE S3 Trio64V+ (generic)

NAME STB Powergraph 64
SEE S3 Trio64 (generic)

NAME ELSA Winner 1000TRIO
SEE S3 Trio64 (generic)

NAME ELSA Winner 1000TRIO/V
SEE S3 Trio64V+ (generic)

NAME Hercules Graphite Terminator 64
LINE     Option "slow_vram"
LINE    #s3RefClk  50
LINE    #DACspeed 170
SEE S3 964 (generic)

NAME Hercules Terminator 64/Video
SEE S3 Trio64V+ (generic)

NAME Hercules Graphite Terminator 64/DRAM
SEE S3 Trio64 (generic)

NAME Hercules Graphite Terminator Pro 64
LINE    #s3RefClk  16
LINE    #DACspeed 220
SEE S3 968 (generic)

NAME Number Nine FX Motion 771
LINE    #s3RefClk  16
SEE S3 968 (generic)

NAME Spider Tarantula 64
SEE S3 964 (generic)

NAME Miro Crystal 20SV
CHIPSET S3 964
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2061a

NAME Miro Crystal 40SV
CHIPSET S3 964
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP ti3025

NAME Miro Crystal 80SV
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME Miro Video 20SV
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c505
LINE    #DacSpeed 150
CLOCKCHIP ics9161a

NAME SPEA Mercury 64
CHIPSET S3 964
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP ics9161a
LINE     #Option "spea_mercury"

NAME ELSA Winner 2000PRO-2
CHIPSET S3 964
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Option "ELSA_w2000pro"
NOCLOCKPROBE

NAME ELSA Winner 2000PRO-4
CHIPSET S3 964
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Option "ELSA_w2000pro"
NOCLOCKPROBE

NAME ELSA Winner 2000PRO/X-2
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Option "sync_on_green"
NOCLOCKPROBE

NAME ELSA Winner 2000PRO/X-4
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Option "sync_on_green"
NOCLOCKPROBE

NAME ELSA Winner 2000PRO/X-8
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Option "sync_on_green"
NOCLOCKPROBE

NAME ELSA Winner 2000AVI
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Option "sync_on_green"
NOCLOCKPROBE

NAME ELSA Gloria-4
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Option "sync_on_green"
NOCLOCKPROBE

NAME ELSA Gloria-8
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Option "sync_on_green"
NOCLOCKPROBE

NAME VideoLogic GrafixStar 700
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME LeadTek WinFast S430
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME WinFast S430
SEE LeadTek WinFast S430

NAME LeadTek WinFast S510
CHIPSET S3 968
SERVER S3
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME WinFast S510
SEE LeadTek WinFast S510

# S3 928

NAME S3 928 (generic)
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED

NAME S3 86C928 (generic)
SEE S3 928 (generic)

NAME Actix Ultra
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC att20c490
LINE     #Option "dac_8_bit"

NAME Diamond Stealth Pro
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2061a
LINE     #Ramdac "att20c490" # The Diamond RAMDAC is reportedly compatible for 15bpp
LINE     #Option "no_linear" # Some VLB machines may require this

NAME ELSA Winner 1000VL
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     # the following settings should be detected and set automatically by XF86_S3
LINE     # if the serial number of the ELSA card is printed correctly:
LINE     #ClockChip "icd2061a"
LINE     #Membase 0xf8000000

NAME ELSA Winner 1000TwinBus
SEE ELSA Winner 1000VL

NAME ELSA Winner 2000
SEE S3 928 (generic)

NAME Miro Crystal 16S
SEE S3 928 (generic)

NAME SPEA/V7 Mercury
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP sc11412
LINE     Option "spea_mercury"

NAME STB Pegasus
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED
RAMDAC bt485
CLOCKCHIP icd2061a
LINE     Option "stb_pegasus"
LINE     #Option "sync_on_green"

NAME Number Nine GXE Level 14/16
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED
DACSPEED 200
CLOCKCHIP icd2061a
LINE     Option "number_nine"
LINE     #Option "nolinear"
LINE     #Option "nomemaccess"

NAME Number Nine GXE Level 10/11/12
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2061a
LINE     Option "number_nine"

NAME 928Movie
CHIPSET S3 928
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2595
RAMDAC bt485
LINE     # pixel multiplexing not supported

# S3 911/924

NAME S3 911/924 (generic)
CHIPSET S3 911/924
SERVER S3
DRIVER vga
UNSUPPORTED

NAME S3 86C911 (generic)
SEE S3 911/924 (generic)

NAME S3 86C924 (generic)
SEE S3 911/924 (generic)

NAME Diamond Stealth VRAM
CHIPSET S3 911/924
SERVER S3
DRIVER vga
UNSUPPORTED
CLOCKCHIP icd2061a

#NAME Orchid Fahrenheit 1280
#SEE S3 911/924 (generic)

NAME S3 924 with SC1148 DAC
CHIPSET S3 924
SERVER S3
DRIVER vga
UNSUPPORTED
LINE     #Probable clocks:
LINE     #Clocks 25.2 28.3 39.7 1.7 49.9 76.7 35.7 44
LINE     #Clocks 130.2 119.5 79.4 31.2 110.0 65.2 74.9 71.3

# S3 ViRGE,/DX,/GX and ViRGE/VX

NAME S3 ViRGE (old S3V server)
CHIPSET S3 ViRGE
SERVER S3V
DRIVER s3virge
NOCLOCKPROBE

NAME S3 ViRGE (generic)
CHIPSET S3 ViRGE
SERVER SVGA
DRIVER s3virge
NOCLOCKPROBE
LINE      #Option "xaa_benchmark"
LINE      #Option "fifo_moderate"
LINE      #Option "pci_burst_on"
LINE      #Option "pci_retry"

NAME S3 ViRGE/DX (generic)
CHIPSET S3 ViRGE/DX
SERVER SVGA
DRIVER s3virge
NOCLOCKPROBE
LINE      #Option "xaa_benchmark"
LINE      #Option "fifo_moderate"
LINE      #Option "pci_burst_on"
LINE      #Option "pci_retry"

NAME S3 ViRGE/GX (generic)
CHIPSET S3 ViRGE/GX
SERVER SVGA
DRIVER s3virge
NOCLOCKPROBE
LINE      #Option "xaa_benchmark"
LINE      #Option "fifo_moderate"
LINE      #Option "pci_burst_on"
LINE      #Option "pci_retry"


NAME S3 ViRGE/GX2 (generic)
CHIPSET S3 ViRGE/GX2
SERVER SVGA
DRIVER s3virge
NOCLOCKPROBE
LINE      #Option "xaa_benchmark"
LINE      #Option "fifo_moderate"
LINE      #Option "pci_burst_on"
LINE      #Option "pci_retry"

NAME S3 ViRGE/MX (generic)
CHIPSET S3 ViRGE/MX
SERVER SVGA
DRIVER s3virge
NOCLOCKPROBE
LINE      #Option "lcd_center"
LINE      #Set_LCDClk  <pixel_clock_for_LCD>
LINE      #Option "xaa_benchmark"
LINE      #Option "fifo_moderate"
LINE      #Option "pci_burst_on"
LINE      #Option "pci_retry"

NAME S3 ViRGE/MX+ (generic)
SEE S3 ViRGE/MX (generic)




NAME S3 86C325 (generic)
SEE S3 ViRGE (generic)

NAME S3 86C375 (generic)
SEE S3 ViRGE/DX (generic)

NAME S3 86C385 (generic)
SEE S3 ViRGE/GX (generic)

NAME S3 86C357 (generic)
SEE S3 ViRGE/GX2 (generic)

NAME S3 86C260 (generic)
SEE S3 ViRGE/MX (generic)

NAME S3 86C280 (generic)
SEE S3 ViRGE/MX+ (generic)


NAME ELSA Victory 3D
SEE S3 ViRGE (generic)

NAME ELSA Victory 3DX
SEE S3 ViRGE/DX (generic)

NAME ELSA Winner 3000-S
SEE S3 ViRGE (generic)

NAME Number Nine Visual 9FX Reality 332
SEE S3 ViRGE (generic)

NAME Number Nine FX Motion 332
SEE S3 ViRGE (generic)

NAME Diamond Stealth 3D 2000
SEE S3 ViRGE (generic)

NAME Diamond Stealth 3D 2000 PRO
SEE S3 ViRGE/DX (generic)

NAME Diamond Multimedia Stealth 3D 2000
SEE S3 ViRGE (generic)

NAME Diamond Multimedia Stealth 3D 2000 PRO
SEE S3 ViRGE/DX (generic)

NAME Canopus Co. Power Window 3DV
SEE S3 ViRGE (generic)

NAME DataExpert DSV3325
SEE S3 ViRGE (generic)

NAME ExpertColor DSV3325
SEE S3 ViRGE (generic)

NAME DSV3325
SEE S3 ViRGE (generic)

NAME Hercules Terminator 64/3D
SEE S3 ViRGE (generic)

NAME Hercules Terminator 3D/DX
SEE S3 ViRGE/DX (generic)

NAME LeadTek WinFast 3D S600
SEE S3 ViRGE (generic)

NAME WinFast 3D S600
SEE LeadTek WinFast 3D S600

NAME LeadTek WinFast 3D S680
SEE S3 ViRGE/GX2 (generic)

NAME Miro MiroMedia 3D
SEE S3 ViRGE (generic)

NAME Orchid Technology Fahrenheit Video 3D
SEE S3 ViRGE (generic)

NAME STB Systems Powergraph 3D
SEE S3 ViRGE (generic)

NAME STB Nitro 3D
CHIPSET S3 ViRGE/GX
SEE S3 ViRGE/GX (generic)

NAME MELCO WGP-VG4S
LINE      #DACSpeed  191 162 111 83
LINE      #SetMClck  75
SEE S3 ViRGE (generic)



NAME S3 ViRGE/VX (generic)
CHIPSET S3 ViRGE/VX
SERVER SVGA
DRIVER s3virge
NOCLOCKPROBE
LINE      #Option "xaa_benchmark"
LINE      #Option "fifo_moderate"
LINE      #Option "pci_burst_on"
LINE      #Option "pci_retry"


NAME S3 86C988 (generic)
SEE S3 ViRGE/VX (generic)

NAME ELSA Winner 3000
SEE S3 ViRGE/VX (generic)

NAME ELSA Winner 3000-M-22
SEE S3 ViRGE/VX (generic)

NAME ELSA Winner 3000-L-42
SEE S3 ViRGE/VX (generic)

NAME ELSA Winner 2000AVI/3D
SEE S3 ViRGE/VX (generic)

NAME Diamond Stealth 3D 3000
SEE S3 ViRGE/VX (generic)

NAME STB Systems Velocity 3D
SEE S3 ViRGE/VX (generic)

NAME MELCO WGP-VX8
SEE S3 ViRGE/VX (generic)

NAME Diamond Stealth 3D 4000
SEE S3 ViRGE/GX2 (generic)

NAME Toshiba Tecra 750CDT
SEE S3 ViRGE/MX (generic)

NAME Toshiba Tecra 750DVD
SEE S3 ViRGE/MX (generic)

NAME Toshiba Tecra 540CDT
SEE S3 ViRGE/MX (generic)

NAME Toshiba Tecra 550CDT
SEE S3 ViRGE/MX (generic)

# currently unsupported S3

NAME S3 86C365 (Trio3D)
SEE * Unsupported VGA compatible

NAME S3 86C391 (Savage3D)
SEE * Unsupported VGA compatible

NAME S3 Trio3D
SEE * Unsupported VGA compatible

NAME S3 Savage3D
SEE * Unsupported VGA compatible

NAME S3 Savage4
SERVER SVGA
DRIVER vga
UNSUPPORTED

# ET4000/ET6000

NAME ET3000 (generic)
CHIPSET ET3000
SERVER SVGA
DRIVER tseng

NAME Genoa 5400
SEE ET3000 (generic)

NAME ET4000 (generic)
CHIPSET ET4000
SERVER SVGA
DRIVER tseng

NAME ET4000/W32 (generic)
CHIPSET ET4000/W32
SERVER W32
DRIVER tseng

NAME ET4000 W32i, W32p (generic)
CHIPSET ET4000/W32(i/p)
SERVER SVGA
DRIVER tseng
LINE     #Option "linear"       # for linear mode at 8bpp
LINE     #Option "noaccel"      # when problems with accelerator
LINE     #Option "power_saver"  # enable VESA DPMS
LINE     #Option "fast_dram"
LINE     #Option "pci_retry"    # faster, but problematic for ISA DMA
LINE     #Option "hibit_high"   # see README.tseng -- most cards need this
LINE     #Option "hibit_low"    # see README.tseng -- mostly for older ET4000 cards
LINE     #MemBase 0x3C00000     # when automatic MemBase detection doesn't work
LINE         # -- see README.tseng for more (important) information on MemBase

NAME ET6000 (generic)
CHIPSET ET6000
SERVER SVGA
DRIVER tseng
NOCLOCKPROBE
LINE     #videoram 2304         # 2.25 MB, when memory probe is incorrect
LINE     #Option "linear"       # for linear mode at 8bpp
LINE     #Option "noaccel"      # when problems with accelerator
LINE     #Option "power_saver"  # enable VESA DPMS
LINE     #Option "pci_retry"    # faster, but problematic for ISA DMA
LINE     #Option "hw_cursor"    # Use hardware cursor (see docs for limitations)
LINE     #Option "xaa_no_color_exp"  # When text (or bitmap) is not rendered correctly

NAME ET6100 (generic)
CHIPSET ET6100
SEE ET6000 (generic)

NAME Diamond Stealth 32
CLOCKCHIP icd2061a
NOCLOCKPROBE
SEE ET4000 W32i, W32p (generic)

NAME Cardex Cobra
SEE ET4000 W32i, W32p (generic)

NAME Cardex Challenger (Pro)
SEE ET4000 W32i, W32p (generic)

NAME Colorgraphic Dual Lightning
SEE ET4000 W32i, W32p (generic)

NAME Dell onboard ET4000
SEE ET4000 (generic)

NAME DFI-WG5000
SEE ET4000 W32i, W32p (generic)

NAME Diamond SpeedStar (Plus)
SEE ET4000 (generic)

NAME Diamond SpeedStar 24
SEE ET4000 (generic)

NAME Diamond SpeedStar HiColor
SEE ET4000 (generic)

NAME Genoa 8900 Phantom 32i
SEE ET4000 W32i, W32p (generic)

NAME Hercules Dynamite
SEE ET4000/W32 (generic)

NAME Hercules Dynamite Power
SEE ET4000 W32i, W32p (generic)

NAME Hercules Dynamite Pro
SEE ET4000 W32i, W32p (generic)

NAME Integral FlashPoint
SEE ET4000 W32i, W32p (generic)

NAME LeadTek WinFast S200
SEE ET4000 W32i, W32p (generic)

NAME Matrox Comet
SEE ET4000 W32i, W32p (generic)

NAME Matrox Marvel II
SEE ET4000 W32i, W32p (generic)

NAME Miro MiroVideo 20TD
SEE ET4000 W32i, W32p (generic)

NAME WinFast S200
SEE LeadTek WinFast S200

NAME Sigma Concorde
SEE ET4000/W32 (generic)

NAME Sigma Legend
SEE ET4000 (generic)

NAME SPEA/V7 ShowTime Plus
SEE ET4000 W32i, W32p (generic)

NAME STB LightSpeed
SEE ET4000 W32i, W32p (generic)

NAME STB MVP-2
SEE ET4000 (generic)

NAME STB MVP-2 PCI
SEE ET4000 W32i, W32p (generic)

NAME STB MVP-2X
SEE ET4000 W32i, W32p (generic)

NAME STB MVP-4 PCI
SEE ET4000 W32i, W32p (generic)

NAME STB MVP-4X
SEE ET4000 W32i, W32p (generic)

NAME TechWorks Thunderbolt
SEE ET4000/W32 (generic)

NAME ViewTop PCI
SEE ET4000 W32i, W32p (generic)

NAME SNI PC5H W32
CLOCKCHIP stg1703
NOCLOCKPROBE
SEE ET4000 W32i, W32p (generic)

NAME SNI Scenic W32
CLOCKCHIP stg1703
NOCLOCKPROBE
SEE ET4000 W32i, W32p (generic)

NAME Hercules Dynamite 128/Video
SEE ET6000 (generic)

NAME STB LightSpeed 128
SEE ET6000 (generic)

NAME VideoLogic GrafixStar 600
SEE ET6000 (generic)

NAME Jazz Multimedia G-Force 128
SEE ET6000 (generic)

NAME Mirage Z-128
SEE ET6000 (generic)

NAME California Graphics SunTracer 6000
SEE ET6000 (generic)

NAME Binar Graphics AnyView
SEE ET6000 (generic)

NAME MediaVision Proaxcel 128
SEE ET6000 (generic)

NAME ATrend ATC-2165A
SEE ET6000 (generic)

NAME Interay PMC Viper
SEE ET6000 (generic)

NAME 2-the-Max MAXColor 6000
SEE ET6000 (generic)

NAME Gainward Challenger EV
SEE ET6000 (generic)

NAME MachSpeed VGA ET6000
SEE ET6000 (generic)

NAME KouTech KeyVision 128 EV
SEE ET6000 (generic)

NAME Jaton Video-58P
SEE ET6000 (generic)

# ATI

NAME ATI Rage 128
CHIPSET ati
SERVER SVGA
DRIVER ati

NAME ATI 8514 Ultra (no VGA)
CHIPSET ati
SERVER Mach8
DRIVER vga
UNSUPPORTED

NAME ATI Graphics Ultra
CHIPSET ati
SERVER Mach8
DRIVER ati

NAME ATI Graphics Ultra Pro
CHIPSET ati
SERVER Mach32
DRIVER ati

NAME ATI Wonder SVGA
CHIPSET ati
SERVER SVGA
DRIVER ati

NAME ATI Ultra Plus
CHIPSET ati
SERVER Mach32
DRIVER ati

NAME ATI Mach32
CHIPSET ati
SERVER Mach32
DRIVER ati

NAME ATI Mach64
CHIPSET ati
SERVER Mach64
DRIVER ati
NOCLOCKPROBE

NAME ATI Mach64 CT (264CT)
SEE ATI Mach64

NAME ATI Mach64 VT (264VT)
SEE ATI Mach64

NAME ATI Mach64 GT (264GT), aka 3D RAGE
SEE ATI Mach64

NAME ATI Mach64 3D RAGE II
SEE ATI Mach64

NAME ATI Mach64 3D RAGE II+DVD
SEE ATI Mach64

NAME ATI Mach64 3D Rage IIC
SEE ATI Mach64

NAME ATI Mach64 3D Rage Pro
SEE ATI Mach64

NAME ATI 3D Pro Turbo
SEE ATI Mach64

NAME ATI 3D Pro Turbo PC2TV
SEE ATI Mach64

NAME ATI 3D Xpression
SEE ATI Mach64

NAME ATI 3D Xpression+
SEE ATI Mach64

NAME ATI 3D Xpression+ PC2TV
SEE ATI Mach64

NAME ATI All-in-Wonder
SEE ATI Mach64

NAME ATI All-in-Wonder Pro
SEE ATI Mach64

NAME ATI Graphics Pro Turbo
SEE ATI Mach64

NAME ATI Graphics Pro Turbo 1600
SEE ATI Mach64

NAME ATI Graphics Xpression
SEE ATI Mach64

NAME ATI Video Boost
SEE ATI Mach64

NAME ATI Video Charger
SEE ATI Mach64

NAME ATI Video Xpression
SEE ATI Mach64

NAME ATI Video Xpression+
SEE ATI Mach64

NAME ATI WinBoost
SEE ATI Mach64

NAME ATI WinCharger
SEE ATI Mach64

NAME ATI WinTurbo
SEE ATI Mach64

NAME ATI Xpert 98
SEE ATI Mach64

NAME ATI Xpert XL
SEE ATI Mach64

NAME ATI Xpert@Play
SEE ATI Mach64

NAME ATI Xpert@Play 98
SEE ATI Mach64

NAME ATI Xpert@Work
SEE ATI Mach64

NAME ATI integrated on Intel Maui MU440EX motherboard
SEE ATI Mach64

NAME ASUS PCI-V264CT
SEE ATI Mach64

NAME ASUS PCI-AV264CT
SEE ATI Mach64

# AGX

NAME AGX (generic)
CHIPSET AGX-014/15/16
SERVER AGX
DRIVER vga
UNSUPPORTED

NAME Boca Vortex (Sierra RAMDAC)
CHIPSET AGX-015
SERVER AGX
DRIVER vga
UNSUPPORTED
RAMDAC sc15025
LINE     Option "dac_8_bit"
LINE     Option "no_wait_state"
LINE     #Option "fifo_moderate"   # 2x bus bw - may result in random pixels

NAME EIZO (VRAM)
SEE AGX (generic)

NAME Orchid Celsius (AT&T RAMDAC)
CHIPSET AGX-015
SERVER AGX
DRIVER vga
UNSUPPORTED
RAMDAC att20c490
LINE     Option "dac_8_bit"
LINE     Option "no_wait_state"
LINE     #Option "fifo_moderate"   # 2x bus bw - may result in random pixels

NAME Orchid Celsius (Sierra RAMDAC)
CHIPSET AGX-015
SERVER AGX
DRIVER vga
UNSUPPORTED
RAMDAC sc15025
LINE     Option "dac_8_bit"
LINE     Option "no_wait_state"
LINE     #Option "fifo_moderate"   # 2x bus bw - may result in random pixels


NAME Spider Black Widow
CHIPSET AGX-015
SERVER AGX
DRIVER vga
UNSUPPORTED
RAMDAC sc15025
LINE     Option "dac_8_bit"
LINE     Option "no_wait_state"
LINE     #Option "fifo_moderate"   # 2x bus bw - may result in random pixels


NAME Spider Black Widow Plus
CHIPSET AGX-016
SERVER AGX
DRIVER vga
UNSUPPORTED
RAMDAC sc15025
LINE     Option "dac_8_bit"
LINE     Option "no_wait_state"
LINE     #Option "fifo_moderate"   # 2x bus bw - may result in random pixels
LINE     #Option "fifo_aggressive" # 3x bus bw - may result in random pixels
LINE	 #Probable clocks:
LINE     #Clocks 25.2  28.3  39.9  72.2  50.0  76.9  36.1  44.8
LINE     #Clocks 89.0  119.8 79.9  31.5 110.0  64.9  74.9  94.9

NAME Hercules Graphite HG210
CHIPSET AGX-014
SERVER AGX
DRIVER vga
UNSUPPORTED
RAMDAC bt482
DACSPEED 85
LINE     Chipset "AGX-014"
LINE     Option "dac_8_bit"
LINE     Option "no_wait_state"
LINE     #Probable clocks:
LINE     #Clocks 25.0  28.0  32.0  36.0  40.0  45.0  50.0  65.0
LINE     #Clocks 70.0  75.0  80.0  85.0  90.0  95.0 100.0 110.0

NAME Hercules Graphite Pro
CHIPSET AGX-015
SERVER AGX
DRIVER vga
UNSUPPORTED
# Card specific DAC, doesn't appear in ramdac menu
LINE     Ramdac "herc_dual_dac"
LINE     Chipset "AGX-015"
LINE     Option "dac_8_bit"
LINE     Option "no_wait_state"
LINE     #Option "fifo_moderate"   # 2x bus bw - may result in random pixels
LINE     #Probable clocks:
LINE     #Clocks 25.0  28.0  32.0  36.0  40.0  45.0  50.0  65.0
LINE     #Clocks 70.0  75.0  80.0  85.0  90.0  95.0 100.0 110.0

NAME Hercules Graphite Power
CHIPSET AGX-016
SERVER AGX
DRIVER vga
UNSUPPORTED
# Card specific DAC, doesn't appear in ramdac menu
#   The glue logic state machine for RAMDAC switching doesn't work as
#   documented, for now we're stuck with the small RAMDAC
LINE     Ramdac "herc_small_dac"
LINE     Chipset "AGX-016"
LINE     Option "dac_8_bit"
LINE     Option "no_wait_state"
LINE     #Option "fifo_moderate"   # 2x bus bw - may result in random pixels
LINE     #Option "fifo_aggressive" # 3x bus bw - may result in random pixels
LINE     #Probable clocks:
LINE     #Clocks 25.0  28.0  32.0  36.0  40.0  45.0  50.0  65.0
LINE     #Clocks 70.0  75.0  80.0  85.0  90.0  95.0 100.0 110.0

NAME XGA-2  (ISA bus)
CHIPSET XGA-2
SERVER AGX
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE
LINE     #Instance  7           # XGA instance 0-7
LINE     #COPbase   0xC8F00     # XGA memory-mapped register address
LINE     #POSbase   0           # Disable probing if above are specified

NAME XGA-1  (ISA bus)
CHIPSET XGA-1
SERVER AGX
DRIVER vga
UNSUPPORTED
LINE     #Instance  7           # XGA instance 0-7
LINE     #COPbase   0xC8F00     # XGA memory-mapped register address
LINE     #POSbase   0           # Disable probing if above are specified

# WD

NAME Paradise/WD 90CXX
CHIPSET WD90CXX
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME DFI-WG6000
CHIPSET WD90C33
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Diamond SpeedStar 24X (not fully supported)
CHIPSET WD90C31
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME WD 90C24 (laptop)
CHIPSET WD90C24
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE     #Chipset "wd90c24"
LINE     #Option "noaccel" # Use this if acceleration is causing problems
LINE     #Clocks 25.175 28.322 65     36     # These are not programmable
LINE     #Clocks 29.979 77.408 62.195 59.957 # These are programmable
LINE     #Clocks 31.5   35.501 75.166 50.114 # These are not programmable
LINE     #Clocks 39.822 72.038 44.744 80.092 # These are programmable
LINE     #Clocks 44.297                      # Must match Mclk


NAME WD 90C24A or 90C24A2 (laptop)
CHIPSET WD90C24A
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE     #Chipset "wd90c24"
LINE     #Clocks 25.175 28.322 65     36     # These are not programmable
LINE     #Clocks 29.979 77.408 62.195 59.957 # These are programmable
LINE     #Clocks 31.5   35.501 75.166 50.114 # These are not programmable
LINE     #Clocks 39.822 72.038 44.744 80.092 # These are programmable
LINE     #Clocks 44.297                      # Must match Mclk

# Avance Logic

NAME Avance Logic 2101
CHIPSET Avance Logic
LINE   #chipset "al2101"
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Avance Logic 2228
CHIPSET Avance Logic
LINE   #chipset "ali2228"
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Avance Logic 2301
CHIPSET Avance Logic
LINE   #chipset "ali2301"
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Avance Logic 2302
CHIPSET Avance Logic
LINE   #chipset "ali2302"
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Avance Logic 2308
CHIPSET Avance Logic
LINE   #chipset "ali2308"
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Avance Logic 2401
CHIPSET Avance Logic
LINE   #chipset "ali2401"
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Hercules Stingray
CHIPSET ALG-2228/2301/2302
LINE   #chipset "ali2228"
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME SPEA/V7 Mirage VEGA Plus
CHIPSET ALG-2228
LINE   #chipset "ali2228"
SERVER SVGA
DRIVER vga
UNSUPPORTED

# ARK Logic

NAME Ark Logic ARK1000PV (generic)
CHIPSET ARK1000PV
SERVER SVGA
DRIVER vga
UNSUPPORTED

# For now, treat the VL as a PV.  This may be changed later
NAME Ark Logic ARK1000VL (generic)
CHIPSET ARK1000VL
LINE Chipset "ark1000pv"
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Ark Logic ARK2000PV (generic)
CHIPSET ARK1000PV
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Ark Logic ARK2000MT (generic)
CHIPSET ARK1000MT
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Hercules Stingray Pro
SEE Ark Logic ARK1000PV (generic)

NAME Hercules Stingray Pro/V
SEE Ark Logic ARK1000PV (generic)

NAME Ocean (octek) VL-VGA-1000
RAMDAC att20c490
SEE Ark Logic ARK1000VL (generic)

NAME Hercules Stingray 64/V with ZoomDAC
SEE Ark Logic ARK2000PV (generic)

NAME Hercules Stingray 64/V with ICS5342
CHIPSET ARK2000MT
RAMDAC ics5342
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Diamond Stealth64 Graphics 2001 series
CHIPSET ARK2000PV
RAMDAC ics5342
SERVER SVGA
DRIVER vga
UNSUPPORTED

# Oak

NAME Oak ISA Card (generic)
CHIPSET Oak OTI-067/77
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Oak 87 VLB (generic)
CHIPSET Oak OTI-087
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE Option "fifo_aggressive" # Comment this if you experience streaks.
LINE Option "no_wait"         # Comment this if you find problems.        
LINE #Option "enable_bitblt"  # You may enable this and see if it works (see README.Oak file)

NAME Oak 87 ISA (generic)
CHIPSET Oak OTI-087
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE Option "noaccel"        # ISA cards seem to have Color Expansion support broken
LINE #Option "enable_bitblt" # This should work on ISA, but lets not make it default just in case.

NAME Paradise Accelerator Value
SEE Oak 87 ISA (generic)

# P9000

NAME Diamond Viper VLB 2Mb
CHIPSET Weitek 9000
SERVER P9000
DRIVER vga
UNSUPPORTED
LINE     #Clocks must match the mode clocks (XFree86 3.1 P9000 server)
LINE     #Versions later than 3.1 do not require a clocks line
LINE     Chipset "vipervlb" # Required for some cards which autodetect as PCI
LINE     Videoram 2048      # Required
LINE     Membase 0x80000000 # Optional (0x80000000 is default)
NOCLOCKPROBE

NAME Diamond Viper PCI 2Mb
CHIPSET Weitek 9000
SERVER P9000
DRIVER vga
UNSUPPORTED
LINE     #Clocks must match the mode clocks (XFree86 3.1 P9000 server)
LINE     #Versions later than 3.1 do not require a clocks line
LINE     Videoram 2048      # Required
LINE     #Membase 0x80000000 # Use scanpci to get the correct Membase
NOCLOCKPROBE

NAME Orchid P9000 VLB
CHIPSET Weitek 9000
SERVER P9000
DRIVER vga
UNSUPPORTED
LINE     Chipset "orchid_p9000"
LINE     Membase 0xE0000000
NOCLOCKPROBE

# P9100

NAME Weitek P9100 (generic)
CHIPSET Weitek P9100
SERVER SVGA
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME Diamond Viper Pro Video
SEE Weitek P9100 (generic)

# Trident

NAME Trident 8900/9000 (generic)
CHIPSET TVGA8900/9000
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Trident 8900D (generic)
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Trident TVGA9200CXr (generic)
CHIPSET TVGA9200CXr
SERVER SVGA
DRIVER vga
UNSUPPORTED

NAME Trident TGUI9400CXi (generic)
CHIPSET TGUI9400CXi
SERVER SVGA
DRIVER trident

NAME Trident TGUI9420DGi (generic)
CHIPSET TGUI9420DGi
SERVER SVGA
DRIVER trident

NAME Trident TGUI9430DGi (generic)
CHIPSET TGUI9430DGi
SERVER SVGA
DRIVER trident

NAME Trident TGUI9420 (generic)
CHIPSET TGUI9420
DRIVER trident
NOCLOCKPROBE

NAME Trident TGUI9440 (generic)
CHIPSET TGUI9440
DRIVER trident
NOCLOCKPROBE

NAME Trident TGUI9660 (generic)
CHIPSET TGUI9660
DRIVER trident
NOCLOCKPROBE

NAME Trident TGUI9680 (generic)
CHIPSET TGUI9680
DRIVER trident
NOCLOCKPROBE

NAME Trident TGUI9682 (generic)
CHIPSET TGUI9682
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident TGUI9685 (generic)
CHIPSET TGUI9685
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident Cyber 9320 (generic)
CHIPSET Cyber9320
DRIVER trident
NOCLOCKPROBE

NAME Trident Cyber 9382 (generic)
CHIPSET Cyber9382
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident Cyber 9385 (generic)
CHIPSET Cyber9385
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident Cyber 9388 (generic)
CHIPSET Cyber9388
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident Cyber 939a (generic)
CHIPSET Cyber939a
DRIVER trident
NOCLOCKPROBE

NAME Trident Cyber 9397 (generic)
CHIPSET Cyber9397
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident Cyber 9520 (generic)
CHIPSET Cyber9520
DRIVER trident
NOCLOCKPROBE

NAME Trident 3DImage975 (generic)
CHIPSET 3dimage975
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident 3DImage975 AGP (generic)
CHIPSET 3dimage975
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident 3DImage985 (generic)
CHIPSET 3dimage985
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident Providia 9682 (generic)
CHIPSET Providia9682
DRIVER trident
NOCLOCKPROBE

NAME Trident Providia 9685 (generic)
CHIPSET Providia9685
DRIVER trident
NOCLOCKPROBE

NAME Trident TVGA 8800BR
SEE * Generic VGA compatible

NAME Trident TVGA 8800CS
SEE * Generic VGA compatible

NAME Trident CyberBlade (generic)
CHIPSET CyberBlade
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

NAME Trident Blade3D (generic)
CHIPSET Blade3D
SERVER SVGA
DRIVER trident
NOCLOCKPROBE

# SiS

NAME SiS 530
CHIPSET SIS530
SERVER SVGA
DRIVER sis

NAME SiS 620
CHIPSET SIS620
SERVER SVGA
DRIVER sis

NAME SiS SG86C201
CHIPSET SIS86C201
SERVER SVGA
DRIVER sis

NAME SiS SG86C205
CHIPSET SIS86C205
SERVER SVGA
DRIVER sis
LINE     # Option "no_accel" # Use this if acceleration is causing problems
LINE     # Option "fifo_moderate" 
LINE     # Option "fifo_conserv" 
LINE     # Option "fifo_aggressive" 
NOCLOCKPROBE

NAME SiS SG86C215
CHIPSET SIS86C215 
SERVER SVGA
DRIVER sis
LINE     # This is a cheap version of 86c205. I am not sure if acceleration works
LINE     # Option "no_accel" # Use this if acceleration is causing problems
LINE     # Option "no_BitBlt" # Use this if acceleration is causing problems
LINE     # Option "fifo_moderate" 
LINE     # Option "fifo_conserv" 
LINE     # Option "fifo_aggressive" 
NOCLOCKPROBE

NAME SiS SG86C225
CHIPSET SIS86C225
SERVER SVGA
DRIVER sis
LINE     # Option "no_accel" # Use this if acceleration is causing problems
LINE     # Option "fifo_moderate" 
LINE     # Option "fifo_conserv" 
LINE     # Option "fifo_aggressive" 
NOCLOCKPROBE

NAME SiS 5597
CHIPSET SiS5597
SERVER SVGA
DRIVER sis
LINE     # Option "no_accel" # Use this if acceleration is causing problems
LINE     # Option "fifo_moderate" 
LINE     # Option "fifo_conserv" 
LINE     # Option "fifo_aggressive" 
LINE     # Option "fast_vram"
LINE     # Option "pci_burst_on"
LINE     # Option "xaa_benchmark" # DON'T use with "ext_eng_queue" !!!
LINE     # Option "ext_eng_queue" # Turbo-queue. This can cause drawing
LINE                              # errors, but gives some accel
NOCLOCKPROBE

NAME SiS 5598
CHIPSET SIS5598
SERVER SVGA
DRIVER sis
LINE     # Option "no_accel" # Use this if acceleration is causing problems
LINE     # Option "fifo_moderate" 
LINE     # Option "fifo_conserv" 
LINE     # Option "fifo_aggressive" 
LINE     # Option "fast_vram"
LINE     # Option "pci_burst_on"
LINE     # Option "xaa_benchmark" # DON'T use with "ext_eng_queue" !!!
LINE     # Option "ext_eng_queue" # Turbo-queue. This can cause drawing
LINE                              # errors, but gives some accel
NOCLOCKPROBE

NAME SiS 6326
CHIPSET SiS6326
SERVER SVGA
DRIVER sis
LINE     # Option "no_accel" # Use this if acceleration is causing problems
LINE     # Option "fifo_moderate" 
LINE     # Option "fifo_conserv" 
LINE     # Option "fifo_aggressive" 
LINE     # Option "fast_vram"
LINE     # Option "pci_burst_on"
LINE     # Option "xaa_benchmark" # DON'T use with "ext_eng_queue" !!!
LINE     # Option "ext_eng_queue" # Turbo-queue. This can cause drawing 
LINE                              # errors, but gives some accel
NOCLOCKPROBE

NAME MSI MS-4417
SEE SiS 6326

NAME SiS 3D PRO AGP
SEE SiS 6326

NAME Miro Crystal DVD
SEE SiS 6326

NAME PC-Chips M567 Mainboard
SEE SiS 5597

NAME Diamond SpeedStar A50
SEE SiS 6326

# Cyrix

NAME MediaGX
CHIPSET mediagx
SERVER SVGA
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

# Alliance ProMotion

NAME Alliance ProMotion 6422
CHIPSET AP6422
SERVER SVGA
DRIVER vga
UNSUPPORTED

# Number 9 I128

NAME Number Nine Imagine I-128
CHIPSET I128
SERVER I128
DRIVER i128
NOCLOCKPROBE

NAME Number Nine Imagine I-128 Series 2
CHIPSET I128
SERVER I128
DRIVER i128
NOCLOCKPROBE

NAME Number Nine Revolution 3D (T2R)
CHIPSET I128
SERVER I128
DRIVER i128
NOCLOCKPROBE

NAME Number Nine Imagine-128 Revolution IV (T2R4)
CHIPSET I128
SERVER I128
DRIVER i128
NOCLOCKPROBE

# Matrox

NAME Matrox Millennium 2MB
CHIPSET mga2064w
SERVER SVGA
DRIVER mga
LINE VideoRam 2048
NOCLOCKPROBE

NAME Matrox Millennium 4MB
CHIPSET mga2064w
SERVER SVGA
DRIVER mga
LINE VideoRam 4096
NOCLOCKPROBE

NAME Matrox Millennium 8MB
CHIPSET mga2064w
SERVER SVGA
DRIVER mga
LINE VideoRam 8192
NOCLOCKPROBE

NAME Matrox Millennium II 4MB
CHIPSET mga2164w
SERVER SVGA
DRIVER mga
LINE VideoRam 4096
NOCLOCKPROBE

NAME Matrox Millennium II 8MB
CHIPSET mga2164w
SERVER SVGA
DRIVER mga
LINE VideoRam 8192
NOCLOCKPROBE

NAME Matrox Millennium II 16MB
CHIPSET mga2164w
SERVER SVGA
DRIVER mga
LINE VideoRam 16384
NOCLOCKPROBE

NAME Matrox Millennium G200 4MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 4096
NOCLOCKPROBE

NAME Matrox Millennium G200 8MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 8192
NOCLOCKPROBE

NAME Matrox Millennium G200 16MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 16384
NOCLOCKPROBE

NAME Matrox Millennium G200 SD 4MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 4096
LINE # Option "mga_sdram"
NOCLOCKPROBE

NAME Matrox Millennium G200 SD 8MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 8192
LINE # Option "mga_sdram"
NOCLOCKPROBE

NAME Matrox Millennium G200 SD 16MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 16384
LINE # Option "mga_sdram"
NOCLOCKPROBE

NAME Matrox Mystique
CHIPSET mga1064sg
SERVER SVGA
DRIVER mga
NOCLOCKPROBE

NAME Matrox Mystique G200 4MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 4096
NOCLOCKPROBE

NAME Matrox Mystique G200 8MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 8192
NOCLOCKPROBE

NAME Matrox Millennium G400
CHIPSET mgag400
SERVER SVGA
DRIVER mga
NOCLOCKPROBE

NAME Matrox Mystique G200 16MB
CHIPSET mgag200
SERVER SVGA
DRIVER mga
LINE VideoRam 16384
NOCLOCKPROBE

NAME Matrox Productiva G100 4MB
CHIPSET mgag100
SERVER SVGA
DRIVER mga
LINE VideoRam 4096
NOCLOCKPROBE

NAME Matrox Productiva G100 8MB
CHIPSET mgag100
SERVER SVGA
DRIVER mga
LINE VideoRam 8192
NOCLOCKPROBE

# NVIDIA

NAME Diamond Edge 3D
CHIPSET nv1
SERVER SVGA
DRIVER vga
UNSUPPORTED
NOCLOCKPROBE

NAME RIVA128
CHIPSET RIVA128
SERVER SVGA
DRIVER nv
NOCLOCKPROBE

NAME RIVA TNT
CHIPSET RIVATNT
SERVER SVGA
DRIVER nv
NOCLOCKPROBE

NAME RIVA TNT2
CHIPSET RIVATNT2
SERVER SVGA
DRIVER nv
NOCLOCKPROBE

NAME NVIDIA GeForce
CHIPSET GeForce
SERVER SVGA
DRIVER nv
NOCLOCKPROBE

NAME ELSA VICTORY ERAZOR
SEE RIVA128

NAME ELSA Winner 1000 R3D
SEE RIVA128

NAME ELSA ERAZOR II
SEE RIVA TNT

NAME Diamond Viper 330
SEE RIVA128

NAME Diamond Viper 550
SEE RIVA TNT

NAME Diamond Viper 770
SEE RIVA TNT2

NAME STB Velocity 128
SEE RIVA128

NAME STB nvidia 128
SEE RIVA128

NAME STB Velocity 4400
SEE RIVA TNT

NAME ASUS 3Dexplorer
SEE RIVA128

NAME Guillemot Maxi Gamer Xentor
SEE RIVA TNT2

NAME Guillemot Maxi Gamer Xentor 32
SEE RIVA TNT2

NAME Creative Graphics Blaster TNT
SEE RIVA TNT

NAME Creative Graphics Blaster TNT2
SEE RIVA TNT2

# 3Dfx
NAME Voodoo Banshee (generic)
SERVER SVGA
CHIPSET 3dfx Banshee
DRIVER tdfx

NAME Voodoo3 (generic)
SERVER SVGA
CHIPSET 3dfx Voodoo3
DRIVER tdfx

NAME Elsa Victory II
SEE Voodoo Banshee (generic)

NAME Diamond Monster Fusion
SEE Voodoo Banshee (generic)

NAME AOpen PA2010
SEE Voodoo Banshee (generic)

NAME Chaintech Desperado 3F10
SEE Voodoo Banshee (generic)

# 3DLabs

NAME ELSA GLoria-L/MX
CHIPSET GLINT MX
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
NOCLOCKPROBE

NAME ELSA GLoria-L
CHIPSET GLINT 500TX
SERVER 3DLabs
DRIVER glint
NOCLOCKPROBE

NAME ELSA GLoria-XL
CHIPSET GLINT MX
SERVER 3DLabs
DRIVER glint
NOCLOCKPROBE

NAME Diamond Fire GL 3000
CHIPSET GLINT 500TX
SERVER 3DLabs
DRIVER glint
LINE Option "firegl_3000"
NOCLOCKPROBE

NAME ELSA GLoria-S
CHIPSET PERMEDIA
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
LINE #VideoRam 8192
NOCLOCKPROBE

NAME Diamond Fire GL 1000
CHIPSET PERMEDIA
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
LINE #VideoRam 8192
NOCLOCKPROBE

NAME ELSA GLoria Synergy
CHIPSET PERMEDIA 2
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
NOCLOCKPROBE

NAME ELSA Winner 2000/Office
CHIPSET PERMEDIA 2
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
NOCLOCKPROBE

NAME Diamond Fire GL 1000 PRO
CHIPSET PERMEDIA 2
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
NOCLOCKPROBE

NAME Creative Blaster Exxtreme
CHIPSET PERMEDIA 2
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
NOCLOCKPROBE

NAME AccelStar Permedia II AGP
CHIPSET PERMEDIA 2
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
NOCLOCKPROBE

NAME Leadtek WinFast 2300
CHIPSET PERMEDIA 2
SERVER 3DLabs
DRIVER glint
NOCLOCKPROBE

NAME 3DLabs Oxygen GMX
CHIPSET PERMEDIA 2
SERVER 3DLabs
DRIVER glint
LINE #Option "no_accel"
NOCLOCKPROBE

NAME Appian Jeronimo 2000
CHIPSET PERMEDIA 3
SERVER 3DLabs
DRIVER glint
NOCLOCKPROBE

# Alliance Semiconductor

NAME Diamond Stealth Video 2500
CHIPSET Alliance AT24 
SERVER SVGA
DRIVER apm
NOCLOCKPROBE

NAME AT3D
CHIPSET Alliance AT3D
SERVER SVGA
DRIVER apm
NOCLOCKPROBE
LINE #Option "no_accel"

NAME AT25
SEE AT3D

NAME Hercules Stingray 128 3D
SEE AT3D

# NeoMagic

NAME NeoMagic (laptop/notebook)
CHIPSET MagicGraph 128 series
SERVER SVGA
DRIVER neomagic
LINE #    Chipset    "NM2160"
LINE #    IOBase     0xfea00000
LINE #    MemBase    0xfd000000
LINE #    VideoRam   2048
LINE #    DacSpeed   90
LINE #    Option     "linear"
LINE #    Option     "nolinear"
LINE #    Option     "sw_cursor"
LINE #    Option     "hw_cursor"
LINE #    Option     "no_accel"
LINE #    Option     "intern_disp"
LINE #    Option     "extern_disp"
LINE #    Option     "mmio"
LINE #    Option     "no_mmio"
LINE #    Option     "lcd_center"
LINE #    Option     "no_stretch"

# Epson SPC8110

NAME EPSON SPC8110 (CardPC)
CHIPSET SPC8110
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE #    Chipset    "spc8110"
LINE #    MemBase    0x03e00000
LINE #    VideoRam   1024
LINE #    Option     "nolinear"
LINE #    Option     "sw_cursor"
LINE #    Option     "noaccel"
LINE #    Option     "fifo_moderate"
LINE #    Option     "fifo_conservative"

# Silicon Motion, Inc.

NAME Silicon Motion Lynx family
CHIPSET Lynx
SERVER SVGA
DRIVER siliconmotion
NOCLOCKPROBE

# Rendition

NAME Rendition Verite 1000
CHIPSET Verite 1000
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE # Option "sw_cursor"

NAME Rendition Verite 2x00
CHIPSET Verite 2x00
SERVER SVGA
DRIVER vga
UNSUPPORTED
LINE # Option "sw_cursor"

NAME Creative Labs 3D Blaster PCI (Verite 1000)
SEE Rendition Verite 1000

NAME Canopus Total-3D
SEE Rendition Verite 1000

NAME Sierra Screaming 3D
SEE Rendition Verite 1000

NAME Miro CRYSTAL VRX
SEE Rendition Verite 1000

NAME Diamond Stealth II S220
CHIPSET Verite 2100
SEE Rendition Verite 2x00

NAME Hercules Thriller3D
CHIPSET Verite 2200
SEE Rendition Verite 2x00

# Digital

NAME Digital 8-plane TGA (UDB/Multia)
CHIPSET TGA
SERVER TGA
DRIVER tga
RAMDAC Bt485

NAME Digital 8-plane TGA (ZLXp-E1)
CHIPSET TGA
SERVER TGA
DRIVER tga
RAMDAC Bt485

NAME Digital 24-plane TGA (ZLXp-E2)
CHIPSET TGA
SERVER TGA
DRIVER tga
RAMDAC Bt463

NAME Digital 24-plane+3D TGA (ZLXp-E3)
CHIPSET TGA
SERVER TGA
DRIVER tga
RAMDAC Bt463

# i810

NAME Intel 810
SERVER SVGA
DRIVER i810

# i740

NAME Intel 740 (generic)
SERVER SVGA
DRIVER i740

# Misc

END
